# Figure2: schematic with AXI-timer



